Efficiency of common fin shapes

 

